PORT NUMBER:--  
• 18 – MSP (Message Send Protocol)  
• 20 - FTP (File Transfer Protocol) for data transfer  
• 21 – FTP (File Transfer Protocol) for data control  
• 23 – Telnet  
• 22 – SSH - Remote Login Protocol  
• 25 - SMTP (Simple Mail Transfer Protocol) for is   
used for sending mails.  
• 53 – DNS (Domain Name System)  
• 67 – DHCP (Dynamic Host Configuration Protocol) for   
sending data to the server – Bootps  
• 68 – DHCP (Dynamic Host Configuration Protocol) for   
data to the client - Bootpc  
• 80 – HTTP (Hypertext Transfer Protocol)  
• 109 – POP2  
• 110 - POP3 (Post Office Protocol) used for   
receiving mails but it uses log-in process.  
• 119 – NNTP (Network News Transfer Protocol)  
• 137 – NetBIOS Name Service  
• 139 – NetBIOS Datagram Service  
• 143 – IMAP4 (Interim Mail Access Protocol) used for   
receiving mails.  
• 150 – NetBIOS Session Service  
• 161 – SNMP  
• 179 – BGP (Border Gateway Protocol)  
• 389 – LDAP (Lightweight Directory Access Protocol)  
• 443 – HTTPS (HTTP-secure)  
• 546 – DHCP Client  
• 547 – DHCP Server